Sennheiser EW-DX v2.0.0 Crestron Module Information

This module is based on the SSCv2 protocol, which uses HTTPS to provide a secure control connection.

EW-DX devices such as EM2, EM2 Dante, and EM4 Dante support SSCv2 starting from firmware version 4.0.0 and later.

While it is still possible to use the older, unsecured module (v1.1.0), we strongly recommend using the secure communication provided by this updated module.

For any questions or issues, please contact: bizcom-alliances@sennheiser.com
